{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["室内工程"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"室内工程","index":0,"n_rows":24,"n_cols":4,"rows_kept":24,"merged":[[1,0,1,3],[11,0,11,3]],"flags":["formulas_cached_only"]}
["番禺院区保健楼副楼装修主材品牌参考"]
["一、电气安装"]
["序号","设备材料名称","备 选 品 牌","备 注"]
[1,"电线电缆","A:广东电缆  B：番禺电缆  C:庆丰电缆","双塑阻燃"]
[2,"配电箱体","A:ABB   B：施耐德   ","　"]
[3,"漏电、空气开关等元器件","A:施耐德、 B：ABB"]
[4,"开关、插座","A: 施耐德   B:西门子    C:ABB","开关、插座面板颜色按设计要求，（其中开关面板要求纯平设计、部分面板带关、带位置标记）"]
[5,"灯 具","A:东松三雄   B：GE照明   C:索恩照明"]
[6,"光 源","A:东松三雄   B：飞利浦照明   C:欧帝尔照明","LED"]
[7,"公共应急照明","A:东松三雄   B：GE照明   C:索恩照明","灯具、应急电源设备应符合最新的消防认证"]
[8,"电线管材","A:番禺天虹 B：广州一通   C:广州永联盛","　"]
["二、建筑墙板、砖、门、卫浴"]
["序号","设备材料名称","备 选 品 牌","备 注"]
[1,"内、外墙乳胶漆","A: 立邦涂料    B:多乐士","净味"]
[2,"内、外墙乳胶漆底漆","A: 立邦涂料    B:多乐士","净味"]
[3,"瓷砖、厕具","A: 东鹏陶瓷   B:佛山“钻石”牌"]
[4,"不锈钢门","广东省名牌","304材料，管材厚度1.0mm"]
[5,"铝合金门、窗","A: 广铝    B:凤铝","玻璃6mm(单扇窗超一平方需钢化),铝材厚度1.4mm"]
[null,null,"三、给排水、防水、遮阳"]
[1,"给排水","A: 雄塑   B:联塑"]
[2,"防水","911材料","不少于二遍"]
[null,"玻璃钢化粪池","广东省名牌","箱体厚度1.2至1.5cm"]
[null,"耐力板材料","广东省名牌","厚度4.0mm"]
[null,"遮阳不锈钢架","广东省名牌","304材料，管材4cmx6cm,厚度2.0mm"]