{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":50,"n_cols":3,"rows_kept":50,"merged":[[0,0,0,2],[49,0,49,2]],"flags":["formulas_cached_only"]}
["番禺院区保健楼副楼装修主要工程量清单"]
["序号","项目名称","面积/数量"]
[1,"新装铝合金平开窗","约70.73m2"]
[2,"不锈钢门带套","8樘"]
[3,"不锈钢钢门（0.9m*2.5m，0.8m*2.1m）","4套"]
[4,"铝合金门","4套"]
[5,"天花抹灰面油漆","355m2"]
[6,"墙面抹灰面油漆","496m2"]
[7,"屋面板裂缝修补","约26m"]
[8,"阳台栏、楼梯扶手板油漆","27.5m2"]
[9,"其他隔断、房间隔墙","50.8m2"]
[10,"线槽暗装","约1500m"]
[11,"楼层配电箱","2个"]
[12,"配线BV-2.5","约2161.02m"]
[13,"配管PC25","约2530.02m"]
[14,"网线UTP-1061C","约1500m"]
[15,"电话线","约500m"]
[16,"二三孔插座","约112个"]
[17,"电话插座、网络插座","约26个"]
[18,"接线盒","约161个"]
[19,"配线BV-4","约650m"]
[20,"空调专用插座","10个"]
[21,"LED灯盘","22套"]
[22,"吸顶灯","12套"]
[23,"单联单控开关","约18个"]
[24,"排气扇","6台"]
[25,"零星砌砖","约18m2"]
[26,"楼梯间防水","36m2"]
[27,"楼梯间一般抹灰","36m2"]
[28,"阳光板屋面","26m2"]
[29,"楼梯（雨棚1.6米）、大门、房顶雨棚","约35.75m2"]
[30,"加建两层卫生间：使用框架混凝土结构","约占地40m2"]
[31,"天顶粉刷，地面及墙体贴300×300防滑砖","约74m2"]
[32,"卫生间成品隔断（抗倍特板）","约90m2"]
[33,"内墙体瓷砖","约144m2"]
[34,"外墙体瓷砖","约162m2"]
[35,"成品玻璃钢化粪池，型号、规格:8m3","1个"]
[36,"挖化粪池土方及回填","约30m3"]
[37,"高密度聚乙烯缠绕管雨水管，管材规格:DN300mm ，埋设深度:1.OOm以内","60m"]
[38,"排污管UPVC，DN150","约86.6m"]
[39,"塑料管PP-R给水管DN25","约20m"]
[40,"塑料管UPVC排水管DN100","约35m，"]
[41,"成套蹲式大便器","8组"]
[42,"成套小便器，带感应式冲洗阀","4组"]
[43,"铝合金纱窗","约40m2"]
[44,"地面瓷砖","约270m2"]
[45,"清理恢复天面地面，做好排水并使用911防水刷二遍","约140m2"]
[46,"应急灯","10盏"]
[47,"楼层树根、杂物清理","1项"]
["因本次装修包含较多隐蔽工程，在施工过程中如出现超出招标清单数量10%内的，不属增加工程。"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}